\section{Filters}\label{filters}

Filters are a method for calculating a variety of useful quantities from the
field variables as the solution evolves in time, such as time-averaged fields
and extracting the field variables at certain points inside the domain. Each
filter is defined in a \inltt{FILTER} tag inside a \inltt{FILTERS} block which
lies in the main \inltt{NEKTAR} tag. In this section we give an overview of the
modules currently available and how to set up these filters in the session file.

Here is an example \inltt{FILTER}:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="FilterName">
      <PARAM NAME="Param1"> Value1 </PARAM>
      <PARAM NAME="Param2"> Value2 </PARAM>
  </FILTER>
\end{lstlisting}

A filter has a name -- in this case, \inltt{FilterName} -- together with
parameters which are set to user-defined values. Each filter expects different
parameter inputs, although where functionality is similar, the same parameter
names are shared between filter types for consistency. Numerical filter
parameters may be expressions and so may include session parameters defined in
the \inltt{PARAMETERS} section.

Some filters may perform a large number of operations, potentially taking up
a significant percentage of the total simulation time. For this purpose,
the parameter \inltt{IO\_FiltersInfoSteps} is used to set the number of steps
between successive total filter CPU time stats are printed. By default it is
set to 10 times \inltt{IO\_InfoSteps}. If the solver is run with the verbose
\inltt{-v} flag, further information is printed, detailing the CPU time of each
individual filter and percentage of time integration.

In the following we document the filters implemented. Note that some filters are
solver-specific and will therefore only work for a given subset of the available
solvers.

\subsection{Phase sampling}
\begin{notebox}
  This feature is currently only supported for filters derived from the
  FieldConvert filter: AverageFields, MovingAverage, ReynoldsStresses.
\end{notebox}

When analysing certain time-dependent problems, it might be of interest to
activate a filter in a specific physical phase and with a certain period
(for instance, to carry out phase averaging).
The simulation time can be written as
$t = m \mathcal{T} + n_{\mathcal{T}} \mathcal{T}$,
where $m$ is an integer representing the number of periods $\mathcal{T}$
elapsed, and $0 \leq n_{\mathcal{T}} \leq 1$ is the phase.
This feature is not a filter in itself and it is activated by adding the
parameters below to the filter of interest:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} &
    \textbf{Description} \\
    \midrule
    \inltt{PhaseAverage}      & \cmark   &  &
    Feature activation\\
    \inltt{PhaseAveragePeriod}      & \cmark   &  &
    Period $\mathcal{T}$\\
    \inltt{PhaseAveragePhase} & \cmark   &  &
    Phase $n_{\mathcal{T}}$.\\
    \bottomrule
  \end{tabularx}
\end{center}

For instance, to activate phase averaging with a period of $\mathcal{T}=10$
at phase $n_{\mathcal{T}}=0.5$:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="FilterName">
      <PARAM NAME="Param1"> Value1 </PARAM>
      <PARAM NAME="Param2"> Value2 </PARAM>
      <PARAM NAME="PhaseAverage"> True </PARAM>
      <PARAM NAME="PhaseAveragePeriod"> 10 </PARAM>
      <PARAM NAME="PhaseAveragePhase"> 0.5 </PARAM>
  </FILTER>
\end{lstlisting}

Since this feature monitors $n_{\mathcal{T}}$ every \inltt{SampleFrequency},
for best results it is recommended to set \inltt{SampleFrequency}$=1$. \\
The maximum error in sampling phase is $n_{\mathcal{T}, \text{tol}} =
\frac{\Delta t}{ 2\mathcal{T}}\cdot$ \inltt{SampleFrequency}, which is displayed
at the beginning of the simulation if the solver is run with the verbose
\inltt{-v} option.\\
The number of periods elapsed is calculated based on simulation time. Caution
is therefore recommended when modifying time information in the restart field,
because if the new time does not correspond to the same phase, the feature
will produce erroneous results.

\subsection{Aerodynamic forces}\label{filters:AeroForces}

\begin{notebox}
  This filter is only supported for the incompressible Navier-Stokes solver.
\end{notebox}

This filter evaluates the aerodynamic forces along a specific surface. The
forces are projected along the Cartesian axes and the pressure and viscous
contributions are computed in each direction.

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \inltt{session} &
    Prefix of the output filename to which the forces are written.\\
    \inltt{Frequency}       & \xmark   & 1 &
    Number of timesteps after which output is written.\\
    \inltt{Boundary}        & \cmark   & - &
    Boundary surfaces on which the forces are to be evaluated.\\
      \inltt{PivotPoint}   & \xmark  & $(0.\; 0.\; 0.)$ & 
      Pivot Point around which the Moments are calculated. If Doesn't explicitly
      defined by user, the moments will be calculated around the point 
      $\mathbf{X}=(0.\; 0.\; 0.)$\\
    \bottomrule
  \end{tabularx}
\end{center}

An example is given below:

\begin{lstlisting}[style=XMLStyle]
  <FILTER TYPE="AeroForces">
      <PARAM NAME="OutputFile">DragLift</PARAM>
      <PARAM NAME="OutputFrequency">10</PARAM>
      <PARAM NAME="Boundary"> B[1,2] </PARAM>		
      <PARAM NAME="PivotPoint"> 1. 0.1 0. </PARAM>		
  </FILTER>
\end{lstlisting}

During the execution a file named \inltt{DragLift.fce} will be created and the
value of the aerodynamic forces on boundaries 1 and 2, defined in the
\inltt{GEOMETRY} section, will be output every 10 time steps.

\subsubsection{Extension for the SPM formulation}\label{filters:sub:ForcesSPM}

\begin{notebox}
    This filter is only supported for the incompressible Navier-Stokes solver
    with the Smoothed Profile Method.
\end{notebox}

The lack of physical boundaries in the Smoothed Profile Method requires an
alternative formulation to calculate the aerodynamic forces. Since the method
imposes the boundary geometry by adding an impulse to the flow proportional to
the difference between the flow velocity and the expected velocity of the
immersed bodies, the forces in this filter are computed by integrating this
difference where $\Phi \neq 0$~\cite{LuoSPM}:

\begin{equation*}
    \frac{\mathbf{F}^n}{\rho} = \frac{1}{\Delta t} \int_{\Omega}
        \Phi^{n+1}(\mathbf{u^*} - \mathbf{u^n}_p)~\text{d}\Omega
\end{equation*}

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} &
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \inltt{session} &
    Prefix of the output filename to which the forces are written.\\
    \inltt{Frequency}       & \xmark   & 1 &
    Number of timesteps after which the output is written.\\
    \inltt{StartTime}       & \xmark   & 0 &
    Forces before this instant are not written to the output.\\
    \bottomrule
  \end{tabularx}
\end{center}

For instance, a block like the following

\begin{lstlisting}[style=XMLStyle]
  <FILTER TYPE="AeroForcesSPM">
      <PARAM NAME="OutputFile"> Forces </PARAM>
      <PARAM NAME="OutputFrequency"> 10 </PARAM>
      <PARAM NAME="StartTime"> 50.0 </PARAM>
  </FILTER>
\end{lstlisting}

will generate a file called \inltt{Forces.fce} with the values of the forces
in the ($X,Y,Z$) directions, that must be scaled with the density of the
fluid to get the real values. It is important to remark that the computed
values are the sum of all the boundaries defined by $\Phi$.

\subsection{Benchmark}\label{filters:Benchmark}

\begin{notebox}
  This filter is only supported for the Cardiac Electrophysiology Solver.
\end{notebox}

Filter \inltt{Benchmark} records spatially distributed event times for 
    activation and repolarisation (recovert) during a simulation, for
    undertaking benchmark test problems.
\begin{lstlisting}[style=XmlStyle]
<FILTER TYPE="Benchmark">
  <PARAM NAME="ThresholdValue"> -40.0 </PARAM>
  <PARAM NAME="InitialValue">     0.0 </PARAM>
  <PARAM NAME="OutputFile"> benchmark </PARAM>
  <PARAM NAME="StartTime">        0.0 </PARAM>
</FILTER>
\end{lstlisting}
    \begin{itemize}
        \item \inltt{ThresholdValue} specifies the value above which tissue is
            considered to be depolarised and below which is considered
            repolarised.
        \item \inltt{InitialValue} specifies the initial value of the
            activation or repolarisation time map.
        \item \inltt{OutputFile} specifies the base filename of activation and
            repolarisation maps output from the filter. This name is appended
            with the index of the event and the suffix `.fld`.
        \item \inltt{StartTime} (optional) specifies the simulation time at
            which to start detecting events.
    \end{itemize}


\subsection{Cell history points}\label{filters:CellHistoryPoints}

\begin{notebox}
  This filter is only supported for the Cardiac Electrophysiology Solver.
\end{notebox}

Filter \inltt{CellHistoryPoints} writes all cell model states over time at
  fixed points. Can be used along with the \inltt{HistoryPoints} filter to
  record all variables at specific points during a simulation.
\begin{lstlisting}[style=XmlStyle]
<FILTER TYPE="CellHistoryPoints">
    <PARAM NAME="OutputFile">crn.his</PARAM>
    <PARAM NAME="OutputFrequency">1</PARAM>
    <PARAM NAME="Points">
        0.00 0.0 0.0
    </PARAM>
</FILTER>
\end{lstlisting}
    \begin{itemize}
        \item \inltt{OutputFile} specifies the filename to write history data to.
        \item \inltt{OutputFrequency} specifies the number of steps between successive outputs.
        \item \inltt{Points} lists coordinates at which history data is to be recorded.
    \end{itemize}

\subsection{Checkpoint cell model}\label{filters:CheckpointCellModel}

\begin{notebox}
  This filter is only supported for the Cardiac Electrophysiology Solver.
\end{notebox}

   Filter \inltt{CheckpointCellModel} checkpoints the cell model. Can be
    used along with the \inltt{Checkpoint} filter to record complete simulation
    state and regular intervals.
\begin{lstlisting}[style=XmlStyle]
<FILTER TYPE="CheckpointCellModel">
  <PARAM NAME="OutputFile"> session </PARAM>
  <PARAM NAME="OutputFrequency"> 1 </PARAM>
</FILTER>
\end{lstlisting}
    \begin{itemize}
        \item \inltt{OutputFile} (optional) specifies the base filename to use.
    If not specified, the session name is used. Checkpoint files are suffixed with the process ID and the extension `.chk`.
        \item \inltt{OutputFrequency} specifies the number of timesteps between
    checkpoints.
    \end{itemize}

\subsection{Checkpoint fields}
 
The checkpoint filter writes a checkpoint file, containing the instantaneous
state of the solution fields at at given timestep. This can subsequently be used
for restarting the simulation or examining time-dependent behaviour. This
produces a sequence of files, by default named \inltt{session\_*.chk}, where
\inltt{*} is replaced by a counter. The initial condition is written to
\inltt{session\_0.chk}. Existing files are not overwritten, but renamed to e.g.
\inltt{session\_0.bak0.chk}. In case this file already exists, too, the \inltt{chk}-file
is renamed to \inltt{session\_0.bak*.chk} and so on.

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \texttt{session} &
    Prefix of the output filename to which the checkpoints are written.\\
    \inltt{OutputFrequency} & \cmark   & - &
    Number of timesteps after which output is written.\\
    \inltt{OutputStartTime} & \xmark & 0 &
    Specifies the simulation time at which to start writing checkpoint files.\\
    \bottomrule
  \end{tabularx}
\end{center}

For example, to output the fields every 100 timesteps we can specify:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="Checkpoint">
      <PARAM NAME="OutputFile">IntermediateFields</PARAM>
      <PARAM NAME="OutputFrequency">100</PARAM>
      <PARAM NAME="OutputStartTime"> 50.0 </PARAM>
  </FILTER>
\end{lstlisting}

It is also possible to specify the \inltt{OutputStartTime} option based on
the simulation time step. For example, if checkpoint files should only be
written after 500 time steps, one can write
\begin{lstlisting}[style=XMLStyle,gobble=2]
      <PARAM NAME="OutputStartTime"> TimeStep * 500 </PARAM>
\end{lstlisting}

\subsection{Electrogram}\label{filters:Electrogram}

\begin{notebox}
  This filter is only supported for the Cardiac Electrophysiology Solver.
\end{notebox}

Filter \inltt{Electrogram} computes virtual unipolar electrograms at a
     prescribed set of points.
\begin{lstlisting}[style=XmlStyle]
<FILTER TYPE="Electrogram">
  <PARAM NAME="OutputFile"> session </PARAM>
  <PARAM NAME="OutputFrequency"> 1 </PARAM>
  <PARAM NAME="Points">
      0.0  0.5  0.7
      1.0  0.5  0.7
      2.0  0.5  0.7
  </PARAM>
</FILTER>
\end{lstlisting}
    \begin{itemize}
    \item \inltt{OutputFile} (optional) specifies the base filename to use. If
    not specified, the session name is used. The extension `.ecg` is appended if not already specified.
    \item \inltt{OutputFrequency} specifies the number of resolution of the
    electrogram data.
    \item \inltt{Points} specifies a list of coordinates at which electrograms
    are desired. \emph{They must not lie within the domain.}
    \end{itemize}

\subsection{Offset Phase}\label{filters:OffsetPhase}

\begin{notebox}
  This filter is only supported for the Cardiac Electrophysiology Solver.
\end{notebox}

Filter \inltt{OffsetPhase} computes the instantaneous phase of the action potential using a time delay-embedding technique \cite{iyer2001}:\\
\begin{equation*}
	\theta(t) = \textnormal{atan2}[v(t-\tau)-\bar v, v(t) - \bar v].
\end{equation*}

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \inltt{session} &
    Prefix of the output filename to which the phase are written.\\
    \inltt{OutputFrequency} & \cmark   & - &
    Number of timesteps after which output is written.\\
    \inltt{MeanV}           & \xmark   & -57.2986 &
    Specifies the time-averaged AP value ($\bar v$) in mV.\\
    \bottomrule
  \end{tabularx}
\end{center}


\subsection{Hilbert Transform Phase based on FFTW}\label{filters:HilbertPhase}

\begin{notebox}
  This filter is only supported for the Cardiac Electrophysiology Solver. 
  To use this filter, user must build Nektar++ with FFTW library. 
\end{notebox}

Filter \inltt{HilbertFFTPhase} computes the instantaneous phase of the action 
potential by generating an analytic signal, $v(t) + i \mathcal{H}\{v\}(t)$.\\
\begin{equation*}
	\mathcal{H}\{v\}(t) = \frac{1}{\pi} \, \textnormal{p.v.} \int^\infty_{-\infty} \frac{v(\tau)}{t-\tau} \, d\tau,
\end{equation*}
and
\begin{equation*}
	\theta(t) = \textnormal{atan2}[\mathcal{H}\{v-\bar v\}(t), v(t) - \bar v].
\end{equation*}

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \inltt{session} &
    Prefix of the output filename to which the phase are written.\\
    \inltt{OutputFrequency} & \cmark   & - &
    Number of timesteps after which an output is written. 
	It is equal to the sampling frequency for Fourier Transform.\\
	\inltt{WindowSize}      & \cmark   & - &
    Number of output steps taken in each FFT. 
	\textit{Note: output steps $\neq$ timesteps.}\\
	\inltt{OverlapSize}     & \cmark   & - &
    Number of output steps overlapped between each segment.\\
    \inltt{MeanV}           & \xmark   & Time-average &
    Specifies the time-averaged AP value in mV.\\
	\inltt{LinearTransitionOverlap} & \xmark & \inltt{true} &
    \inltt{true}: Use linear transition in overlapping region(s). 
	\inltt{false}: Use simple average in overlapping region(s). 
	Input must be either \inltt{true} or \inltt{false}.\\
    \bottomrule
  \end{tabularx}
\end{center}


\subsection{Error}\label{filters:Error}

This filter produces a file containing the time-evolution of the $L_2$ and
$L_{inf}$ errors. By default this file is called \inltt{session.err} where
\inltt{session} is the session name.

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} &
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \inltt{session} &
    Prefix of the output filename to which the errors are written.\\
    \inltt{OutputFrequency} & \xmark   & 1 &
    Number of timesteps after which output is written.\\
    \inltt{ConsoleOutput} & \xmark   & 0 &
    Also output error in the console when writing to file.\\
    \bottomrule
  \end{tabularx}
\end{center}

An example syntax is given below:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="Error">
      <PARAM NAME="OutputFile">ErrorFile</PARAM>
      <PARAM NAME="OutputFrequency">10</PARAM>
      <PARAM NAME="ConsoleOutput">1</PARAM>
  </FILTER>
\end{lstlisting}

\subsection{Integral}\label{filters:Integral}

This filter produces a file containing the time-evolution of the integral of
the solver variables on user defined composites. By default this file is called
\inltt{session.int} where \inltt{session} is the session name.

The following parameters are supported:

\begin{center}
    \begin{tabularx}{0.99\textwidth}{lllX}
        \toprule
        \textbf{Option name} & \textbf{Required} & \textbf{Default} &
        \textbf{Description} \\
        \midrule
        \inltt{OutputFile}      & \xmark   & \inltt{session} &
        Prefix of the output filename to which the integrals are written.\\
        \inltt{OutputFrequency} & \xmark   & 1 &
        Number of timesteps after which output is written.\\
        \inltt{OutputPrecision} & \xmark   & 7 &
        Decimal precision with which the output is written.\\
        \inltt{Composites} & \cmark   & - &
        Composites on which to calculate the integral.\\
        \bottomrule
    \end{tabularx}
\end{center}

Multiple composites can be defined together by using ranges with each composite
grouping producing a summed output for each variable in the \inltt{OutputFile}.
For example \inltt{C[1,3,5-7]} would produce a single integral output for each
variable whilst \inltt{C[1-3], C[4]} would produce two.

An example syntax is given below:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="Integral">
      <PARAM NAME="OutputFile">IntegralFile</PARAM>
      <PARAM NAME="OutputFrequency">10</PARAM>
      <PARAM NAME="OutputPrecision"> 12 </PARAM>
      <PARAM NAME="Composites"> C[1], C[2-4,6]</PARAM>
  </FILTER>
\end{lstlisting}

\subsection{Integral}\label{filters:Integral}

This filter produces a file containing the time-evolution of the integral of
the solver variables on user defined composites. By default this file is called
\inltt{session.int} where \inltt{session} is the session name.

The following parameters are supported:

\begin{center}
    \begin{tabularx}{0.99\textwidth}{lllX}
        \toprule
        \textbf{Option name} & \textbf{Required} & \textbf{Default} &
        \textbf{Description} \\
        \midrule
        \inltt{OutputFile}      & \xmark   & \inltt{session} &
        Prefix of the output filename to which the integrals are written.\\
        \inltt{OutputFrequency} & \xmark   & 1 &
        Number of timesteps after which output is written.\\
        \inltt{OutputPrecision} & \xmark   & 7 &
        Decimal precision with which the output is written.\\
        \inltt{Composites} & \cmark   & - &
        Composites on which to calculate the integral.\\
        \bottomrule
    \end{tabularx}
\end{center}

Multiple composites can be defined together by using ranges with each composite
grouping producing a summed output for each variable in the \inltt{OutputFile}.
For example \inltt{C[1,3,5-7]} would produce a single integral output for each
variable whilst \inltt{C[1-3], C[4]} would produce two.

An example syntax is given below:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="Integral">
      <PARAM NAME="OutputFile">IntegralFile</PARAM>
      <PARAM NAME="OutputFrequency">10</PARAM>
      <PARAM NAME="OutputPrecision"> 12 </PARAM>
      <PARAM NAME="Composites"> C[1], C[2-4,6]</PARAM>
  </FILTER>
\end{lstlisting}

\subsection{FieldConvert checkpoints}

This filter applies a sequence of FieldConvert modules to the solution, 
writing an output file. An output is produced at the end of the simulation into
\inltt{session\_fc.fld}, or alternatively every $M$ timesteps as defined by the
user, into a sequence of files \inltt{session\_*\_fc.fld}, where \inltt{*} is
replaced by a counter.

Module options are specified as a colon-separated list, following the same syntax as the \inltt{FieldConvert} command-line utility (see Section~\ref{s:utilities:fieldconvert}).

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \texttt{session.fld} &
    Output filename. If no extension is provided, it is assumed as .fld\\
    \inltt{OutputFrequency} & \xmark   & \texttt{NumSteps} &
    Number of timesteps after which output is written, $M$.\\
    \inltt{Modules} & \xmark   &  &
    FieldConvert modules to run, separated by a white space.\\
    \inltt{OutputStartTime} & \xmark & 0 &
    Specifies the simulation time at which to start writing checkpoint files.\\
    \bottomrule
  \end{tabularx}
\end{center}

As an example, consider:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="FieldConvert">
      <PARAM NAME="OutputFile">MyFile.vtu</PARAM>
      <PARAM NAME="OutputFrequency">100</PARAM>      
      <PARAM NAME="OutputStartTime"> 50.0 </PARAM>
      <PARAM NAME="Modules"> vorticity isocontour:fieldid=0:fieldvalue=0.1 </PARAM>
  </FILTER>
\end{lstlisting}

See the Checkpoint fields filter for more details about the \inltt{OutputStartTime} parameter.

This will create a sequence of files named \inltt{MyFile\_*\_fc.vtu} containing isocontours. 
The result will be output every 100 time steps.

\subsection{History points}

The history points filter can be used to evaluate the value of the fields in
specific points of the domain as the solution evolves in time. By default this 
produces a file called \inltt{session.his}. For each timestep, and then each 
history point, a line is output containing the current solution time, followed 
by the value of each of the field variables. Commented lines are created at the
top of the file containing the location of the history points and the order of 
the variables.

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \texttt{session} &
    Prefix of the output filename to which the checkpoints are written.\\
    \inltt{OutputFrequency} & \xmark   & 1 &
    Number of timesteps after which output is written.\\
    \inltt{OutputOneFile}      & \xmark   & \texttt{true} &
    If \inltt{OutputOneFile} is \inltt{true} or \inltt{yes}, only one file is generated for all points and the whole history. Otherwise, a separate file is created for each time snapshot.\\
    \inltt{OutputPlane}     & \xmark   & -1 &
    If the simulation is homogeneous, the plane on which to evaluate the 
    history point. If set, all points will be reset to lie on this plane.\\
     \inltt{WaveSpace}     & \xmark   & false &
    If the simulation is homogeneous and \inltt{WaveSpace} is \inltt{true} or \inltt{yes}, the Fourier coefficient on the nearest plane will be output. \\
    \inltt{Points      }    & \xmark   & - &
    A list of the history points. \\
    \inltt{line      }    & \xmark   & - &
    \inltt{npts,x0,y0,x1,y1} in 2D or \inltt{npts,x0,y0,z0,x1,y1,z1} in 3D. Set the history points as npts equispaced points between (x0,y0,z0) and (x1,y1,z1).\\
    \inltt{plane      }    & \xmark   & - &
    \inltt{npts1,npts2,x0,y0,z0,x1,y1,z1,x2,y2,z2,x3,y3,z3}. Set the history points as \inltt{npts1 * npts2} equispaced points on a plane. \inltt{npts1,npts2} is the number of equispaced points in each
    direction and $(x_0,y_0,z_0)$, $(x_1,y_1,z_1)$, $(x_2,y_2,z_2)$ and
    $(x_3,y_3,z_3)$ define the plane of points specified in a clockwise or
    anticlockwise direction. Be careful about the size of history points file when using this option.\\
    \inltt{box      }    & \xmark   & - &
    \inltt{npts1,npts2,npts3,xmin,xmax,ymin,ymax,zmin,zmax}. Set the history points as \inltt{npts1 * npts2 * npts3} equispaced points in a box. \inltt{npts1,npts2,npts3} is the number of equispaced points in each
    direction and $(x_{min},y_{min},z_{min})$ and $(x_{max},y_{max},z_{max})$
    define the limits of the box of points. Be careful about the size of history points file when using this option.\\
    \bottomrule
  \end{tabularx}
\end{center}
One of \inltt{Points      }, \inltt{line      }, \inltt{plane      } or \inltt{box      } must be specified.

For example, to output the value of the solution fields at three points
$(1,0.5,0)$, $(2,0.5,0)$ and $(3,0.5,0)$ into a file \inltt{TimeValues.his}
every 10 timesteps, we use the syntax:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="HistoryPoints">
      <PARAM NAME="OutputFile">TimeValues</PARAM>
      <PARAM NAME="OutputFrequency">10</PARAM>
      <PARAM NAME="Points">
          1 0.5 0
          2 0.5 0
          3 0.5 0
      </PARAM>
  </FILTER>
\end{lstlisting}
or
\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="HistoryPoints">
      <PARAM NAME="OutputFile">TimeValues</PARAM>
      <PARAM NAME="OutputFrequency">10</PARAM>
      <PARAM NAME="line">3,1,0.5,0,3,0.5,0</PARAM>
  </FILTER>
\end{lstlisting}

\subsection{Kinetic energy and enstrophy}\label{filters:Energy}

\begin{notebox}
  This filter is only supported for the incompressible and compressible
  Navier-Stokes solvers \textbf{in three dimensions}.
\end{notebox}

The purpose of this filter is to calculate the kinetic energy and enstrophy
%
\[
E_k = \frac{1}{2\mu(\Omega)}\int_{\Omega} \|\mathbf{u}\|^2\, dx, \qquad
\mathcal{E} = \frac{1}{2\mu(\Omega)}\int_{\Omega} \|\mathbf{\omega}\|^2\, dx
\]
%
where $\mu(\Omega)$ is the volume of the domain $\Omega$. This produces a file
containing the time-evolution of the kinetic energy and enstrophy fields. By
default this file is called \inltt{session.eny} where \inltt{session} is the
session name.

The following parameters are supported:
%
\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \texttt{session.eny} &
    Output file name to which the energy and enstrophy are written.\\
    \inltt{OutputFrequency} & \cmark   & - &
    Number of timesteps at which output is written.\\
    \bottomrule
  \end{tabularx}
\end{center}
%
To enable the filter, add the following to the \inltt{FILTERS} tag:
%
\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="Energy">
      <PARAM NAME="OutputFrequency"> 1 </PARAM>
  </FILTER>
\end{lstlisting}

\subsection{Mean values}\label{filters:MeanValue}

This filter calculates time-evolution of the averaged velocity components
over the flow domain and can be used to track flow rates.

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \inltt{session} &
    Prefix of the output filename to which averaged values are written.\\
    \inltt{OutputFrequency} & \xmark   & 1 &
    Number of timesteps after which output is written.\\
    \bottomrule
  \end{tabularx}
\end{center}

An example syntax is given below:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="Mean">
      <PARAM NAME="OutputFile">mean</PARAM>
      <PARAM NAME="OutputFrequency">10</PARAM>
  </FILTER>
\end{lstlisting}


\subsection{Modal energy}\label{filters:ModalEnergy}

\begin{notebox}
  This filter is only supported for the incompressible Navier-Stokes solver.
\end{notebox}

This filter calculates the time-evolution of the kinetic energy. In the case of
a two- or three-dimensional simulation this is defined as
\[
E_k(t) = \frac{1}{2} \int_{\Omega} \|\mathbf{u}\|^2\, dx
\]
However if the simulation is written as a one-dimensional homogeneous expansion
so that
\[
\mathbf{u}(\mathbf{x},t) = \sum_{k=0}^N \mathbf{\hat{u}}_k(t)e^{2\pi ik\mathbf{x}}
\]
then we instead calculate the energy spectrum
\[
E_k(t) = \frac{1}{2} \int_{\Omega} \|\mathbf{\hat{u}}_k\|^2\, dx.
\]
Note that in this case, each component of $\mathbf{\hat{u}}_k$ is a complex
number and therefore $N = \inltt{HomModesZ}/2$ lines are output for each
timestep. This is a particularly useful tool in examining turbulent and
transitional flows which use the homogeneous extension. In either case, the
resulting output is written into a file called \inltt{session.mdl} by default.

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \inltt{session} &
    Prefix of the output filename to which the energy spectrum is written.\\
    \inltt{OutputFrequency} & \xmark   & 1 &
    Number of timesteps after which output is written.\\
    \bottomrule
  \end{tabularx}
\end{center}

An example syntax is given below:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="ModalEnergy">
      <PARAM NAME="OutputFile">EnergyFile</PARAM>
      <PARAM NAME="OutputFrequency">10</PARAM>
  </FILTER>
\end{lstlisting}

\subsection{Moving body}\label{filters:MovingBody}

\begin{notebox}
  This filter is only supported for the Quasi-3D incompressible Navier-Stokes
  solver, in conjunction with the MovingBody forcing.
\end{notebox}

This filter \inltt{MovingBody} is encapsulated in the forcing module
to evaluate the aerodynamic forces along the moving body surface.
It is described in detail in section \ref{s:forcing:MovingBody}


\subsection{Moving average of fields}

This filter computes the exponential moving average (in time) of
fields for each variable defined in the session file. The moving average 
is defined as:
\[
\bar{u}_n = \alpha u_n + (1 - \alpha)\bar{u}_{n-1}
\]
with $0 < \alpha < 1$ and $\bar{u}_1 = u_1$.

The same parameters of the time-average filter are supported, with the output file
in the form \inltt{session\_*\_movAvg.fld}. In addition,
either $\alpha$ or the time-constant $\tau$ must be defined. They are related by:
\[
\alpha = \frac{t_s}{\tau + t_s}
\]
where $t_s$ is the time interval between consecutive samples.

As an example, consider:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="MovingAverage">
      <PARAM NAME="OutputFile">MyMovingAverage</PARAM>
      <PARAM NAME="OutputFrequency">100</PARAM>
      <PARAM NAME="SampleFrequency"> 10 </PARAM>
      <PARAM NAME="tau"> 0.1 </PARAM>
  </FILTER>
\end{lstlisting}

This will create a file named \inltt{MyMovingAverage\_movAvg.fld} with a moving average
sampled every 10 time steps. The averaged field is however only
output every 100 time steps.

\subsection{One-dimensional energy}

This filter is designed to output the energy spectrum of one-dimensional
elements. It transforms the solution field at each timestep into a orthogonal
basis defined by the functions
\[
\psi_p(\xi) = L_p(\xi)
\]
where $L_p$ is the $p$-th Legendre polynomial. This can be used to show the
presence of, for example, oscillations in the underlying field due to numerical
instability. The resulting output is written into a file called
\inltt{session.eny} by default. The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} &
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \inltt{session} &
    Prefix of the output filename to which the energy spectrum is written.\\
    \inltt{OutputFrequency} & \xmark   & 1 &
    Number of timesteps after which output is written.\\
    \bottomrule
  \end{tabularx}
\end{center}

An example syntax is given below:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="Energy1D">
      <PARAM NAME="OutputFile">EnergyFile</PARAM>
      <PARAM NAME="OutputFrequency">10</PARAM>
  </FILTER>
\end{lstlisting}

\subsection{Reynolds stresses}\label{filters:ReynoldsStresses}

\begin{notebox}
  This filter is only supported for the incompressible Navier-Stokes solver.
\end{notebox}

This filter is an extended version of the time-average fields filter (see Section~\ref{filters:TimeAveragedFields}). It outputs
not only the time-average of the fields, but also the Reynolds stresses.
The same parameters supported in the time-average case can be used,
for example:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="ReynoldsStresses">
      <PARAM NAME="OutputFile">MyAverageField</PARAM>
      <PARAM NAME="RestartFile">MyAverageRst.fld</PARAM>
      <PARAM NAME="OutputFrequency">100</PARAM>
      <PARAM NAME="SampleFrequency"> 10 </PARAM>
  </FILTER>
\end{lstlisting}

By default, this filter uses a simple average. Optionally, an exponential
moving average can be used, in which case the output contains the moving
averages and the Reynolds stresses calculated based on them. For example:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="ReynoldsStresses">
      <PARAM NAME="OutputFile">MyAverageField</PARAM>
      <PARAM NAME="MovingAverage">true</PARAM>
      <PARAM NAME="OutputFrequency">100</PARAM>
      <PARAM NAME="SampleFrequency"> 10 </PARAM>
      <PARAM NAME="alpha"> 0.01 </PARAM>
  </FILTER>
\end{lstlisting}

\subsection{Time-averaged fields}\label{filters:TimeAveragedFields}

This filter computes time-averaged fields for each variable defined in the
session file. Time averages are computed by either taking a snapshot of the
field every timestep, or alternatively at a user-defined number of timesteps
$N$. An output is produced at the end of the simulation into
\inltt{session\_avg.fld}, or alternatively every $M$ timesteps as defined by the
user, into a sequence of files \inltt{session\_*\_avg.fld}, where \inltt{*} is
replaced by a counter. This latter option can be useful to observe statistical
convergence rates of the averaged variables.

This filter is derived from FieldConvert filter, and therefore support all parameters
available in that case. The following additional parameter is supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{SampleFrequency} & \xmark   & 1 &
    Number of timesteps at which the average is calculated, $N$.\\
    \inltt{RestartFile} & \xmark   &   &
    Restart file used as initial average.
    If no extension is provided, it is assumed as .fld\\
  \end{tabularx}
\end{center}

As an example, consider:

\begin{lstlisting}[style=XMLStyle,gobble=2]
  <FILTER TYPE="AverageFields">
      <PARAM NAME="OutputFile">MyAverageField</PARAM>
      <PARAM NAME="RestartFile">MyRestartAvg.fld</PARAM>
      <PARAM NAME="OutputFrequency">100</PARAM>
      <PARAM NAME="SampleFrequency"> 10 </PARAM>		
  </FILTER>
\end{lstlisting}

This will create a file named \inltt{MyAverageField.fld} averaging the
instantaneous fields every 10 time steps. The averaged field is however only
output every 100 time steps.


\subsection {ThresholdMax}\label{filters:ThresholdMax}

The threshold value filter writes a field output containing a variable $m$,
defined by the time at which the selected variable first exceeds a specified
threshold value. The default name of the output file is the name of the session
with the suffix \inlsh{\_max.fld}. Thresholding is applied based on the first
variable listed in the session by default.

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} & 
    \textbf{Description} \\
    \midrule
    \inltt{OutputFile}      & \xmark   & \emph{session}\_max.fld &
    Output filename to which the threshold times are written.\\
    \inltt{ThresholdVar}    & \xmark   & \emph{first variable name} &
    Specifies the variable on which the threshold will be applied.\\
    \inltt{ThresholdValue}  & \cmark   & - &
    Specifies the threshold value.\\
    \inltt{InitialValue}    & \cmark   & - &
    Specifies the initial time.\\
    \inltt{StartTime}       & \xmark   & 0.0 &
    Specifies the time at which to start recording.\\
    \bottomrule
  \end{tabularx}
\end{center}
 
An example is given below:
 
\begin{lstlisting}[style=XMLStyle]
  <FILTER TYPE="ThresholdMax">
      <PARAM NAME="OutputFile"> threshold_max.fld </PARAM>
      <PARAM NAME="ThresholdVar"> u </PARAM>
      <PARAM NAME="ThresholdValue"> 0.1 </PARAM>
      <PARAM NAME="InitialValue">  0.4 </PARAM>
  </FILTER>
\end{lstlisting}

which produces a field file \inlsh{threshold\_max.fld}.

\subsection{ThresholdMin value}\label{filters:ThresholdMin}

Performs the same function as the \inltt{ThresholdMax} filter (see Section~\ref{filters:ThresholdMax}) but records the
time at which the threshold variable drops below a prescribed value.

\subsection{Maximun/minimun fields}\label{filters:MaxMinFields}

This filter computes the local (pointwise) maximum or minimum field for each
variable, including the addition variables for compressible flow solver, over
the simulation.

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} &
    \textbf{Description} \\
    \midrule
    \inltt{MaxOrMin}        & \cmark   & max &
    Type of fields to compute. It can be either \inltt{max} or \inltt{min}.\\
    \inltt{RestartFile}     & \xmark   & $\mp 9999$ &
    Restart file used for initial comparison. If it is not provided, $-9999$
    will be used for the \inltt{max} filter while $9999$ will be used for the
    \inltt{min} filter.
    Output filename to which the threshold times are written.\\
    \inltt{OutputFile}      & \xmark   & \emph{session}\_max.fld &
    Output filename to which the threshold times are written.\\
    \inltt{OutputFrequency} & \xmark   & 1 &
    Number of timesteps after which output is written.\\
    \inltt{SampleFrequency} & \xmark   & 1 &
    Number of timesteps after which the fields are used to compute max/min.\\
    \bottomrule
  \end{tabularx}
\end{center}

An example is given below:

\begin{lstlisting}[style=XMLStyle]
  <FILTERS>
    <FILTER TYPE="MaxMinFields">
      <PARAM NAME="MaxOrMin">max</PARAM>
      <PARAM NAME="RestartFile">Baseflow.fld</PARAM>
      <PARAM NAME="OutputFile">DisturbedFields</PARAM>
      <PARAM NAME="OutputFrequency">100</PARAM>
      <PARAM NAME="SampleFrequency">1</PARAM>
    </FILTER>                                                                                                                                                                                 
  </FILTERS>
\end{lstlisting}

\subsection{Python script}\label{filters:MaxMinFields}

\begin{notebox}
  This feature is only supported if Python support is enabled with the
  \inltt{NEKTAR\_BUILD\_PYTHON} flag enabled at configuration time.
\end{notebox}

The aim of this filter is to permit the execution of a Python script to
implement more complex programmatic filters, but with the ease-of-use of the
Python environment. Python filters mimic the action of C++ filters, and thus
have three separate phases that should be implemented:
\begin{itemize}
  \item an initialisation phase, which is called when the filter is constructed;
  \item an update phase, which is called typically at the end of a timestep;
  \item a finalise phase, which is called at the end of the simulation.
\end{itemize}

Given a Python file as input, the filter can operate in one of two ways:

\begin{itemize}
  \item If only the Python file is supplied, then \nekpp will try to call three
  Python functions: \inltt{filter\_initialise}, \inltt{filter\_update} and
  \inltt{filter\_finalise}. Each function is passed a list of the
  \inltt{ExpList} fields, and the value of the solver time $t$.
  \item If, in addition to the Python file, a filter name is supplied, then
  \nekpp assumes that your Python file creates a subclass of the \inltt{Filter}
  class which has been registered with the \inltt{Filter} factory.
\end{itemize}

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} &
    \textbf{Description} \\
    \midrule
    \inltt{PythonFile} & \cmark   & - &
    Name of the Python file to load.\\
    \inltt{FilterName} & \xmark   & - &
    Optional name of filter if Python subclass is implemented.\\
    \bottomrule
  \end{tabularx}
\end{center}

An example is given below:

\begin{lstlisting}[style=XMLStyle]
  <FILTERS>
    <!-- Python filter with function approach -->
    <FILTER TYPE="Python">
      <PARAM NAME="PythonFile"> FilterPython_Function.py </PARAM>
    </FILTER>
    <!-- Python filter with class approach -->
    <FILTER TYPE="Python">
      <PARAM NAME="PythonFile"> FilterPython_Class.py </PARAM>
      <PARAM NAME="FilterName"> TestFilter </PARAM>
    </FILTER>
  </FILTERS>
\end{lstlisting}

For the first example, a sample Python script may look something like:

\begin{lstlisting}[style=PythonStyle]
def filter_initialise(fields, time):
    pass

def filter_update(fields, time):
    pass  

def filter_finalise(fields, time):
    pass
\end{lstlisting}

For the second example, we might expect something like:

\begin{lstlisting}[style=PythonStyle]
from NekPy.SolverUtils import Filter

class TestFilter(Filter):
    def __init__(self, session, eqsys, params):
        # Call super's constructor.
        super().__init__(session, eqsys)
        # Counter which is incremented at each timestep.
        self.num = 0

    def Initialise(self, fields, time):
        pass

    def Update(self, fields, time):
        self.num += 1

    def Finalise(self, fields, time):
        # Print for testing purposes
        print(self.num)

    def IsTimeDependent(self):
        return True

# Register filter with factory.
Filter.Register("TestFilter", TestFilter)
\end{lstlisting}

\subsection{Body-fitted velocity fields}\label{filters:BodyFittedVelocity}

The \inltt{BodyFittedVelocity} filter projects the velocity fields in the Cartesian coordinate system into
a body-fitted coordinate system. Meanwhile the user can chose to record the local 
(pointwise) maximum or minimum for the body-fitted velocity components, or simply 
output their original values. This filter is designed for both compressible flow
solver and incompressible flow solver.

The following parameters are supported:

\begin{center}
  \begin{tabularx}{0.99\textwidth}{lllX}
    \toprule
    \textbf{Option name} & \textbf{Required} & \textbf{Default} &
    \textbf{Description} \\
    \midrule
    \inltt{BodyFittedCoordinateFile}   & \cmark   & N/A &
    Body-fitted coordinate system generated by FieldConvert module. See 
    \ref{s:utilities:fieldconvert:sub:bodyFittedVelocity} for reference.\\
    \inltt{RestartFile}                & \cmark   & N/A &
    Restart file for the initial field for body-fitted velocity components
    $u_{bfc}$ and $v_{bfc}$ (and $w_{bfc}$ for 3D cases). This restart file 
    is necessary in the currtnt filter. The restart file can use the same 
    output of the FieldConvert modul as well. See 
    \ref{s:utilities:fieldconvert:sub:bodyFittedVelocity} for reference  \\
    \inltt{OriginalOrMaxOrMin}        & \xmark   & original &
    Type of fields to compute. It can be \inltt{original} or \inltt{max} 
    or \inltt{min}.\\
    \inltt{OutputFile}      & \xmark   & \emph{session}\_max.fld &
    Output filename to which the threshold times are written.\\
    \inltt{OutputFrequency} & \xmark   & 1 &
    Number of timesteps after which output is written.\\
    \inltt{SampleFrequency} & \xmark   & 1 &
    Number of timesteps after which the fields are used to compute 
    original/max/min.\\
  \end{tabularx}
\end{center}

An example is given below:
        
\begin{lstlisting}[style=XMLStyle]
  <FILTERS>
    <FILTER TYPE="BodyFittedVelocity">
      <PARAM NAME="RestartFile">bfcFile.fld</PARAM>
      <PARAM NAME="BodyFittedCoordinateFile">bfcFile.fld</PARAM>
      <PARAM NAME="OriginalOrMaxOrMin">max</PARAM>
      <PARAM NAME="OutputFile">vel_bfc</PARAM>
      <PARAM NAME="OutputFrequency">100</PARAM>
      <PARAM NAME="SampleFrequency">1</PARAM>
    </FILTER>
  </FILTERS>
\end{lstlisting}

\subsection{Lagrangian points Tracking}\label{filters:LagrangianPoints}

The \inltt{FilterLagrangianPoints} filter tracks Lagrangian points in parallel. The following parameters are supported:
\begin{center}
    \begin{tabularx}{0.99\textwidth}{lllX}
        \toprule
        \textbf{Option name} & \textbf{Required} & \textbf{Default} &
        \textbf{Description} \\
        \midrule
        \inltt{OutputFile}   & \xmark   & Session name &
        OutputFile\_R\%05d\_T\%010.6lf.plt is output file name for the Lagrangian points. R is followed by the thread number and T is followed by the instantaneous time.\\
        \inltt{OutputFrequency}                & \xmark   & 1 &
        Output frequency of the Lagrangian points.  \\
        \inltt{Box\_n}        & \cmark   & N/A &
        Box\_n = Nx,Ny,Nz, xmin,xmax, ymin,ymax, zmin,zmax. Points defined by a box that initially owned by the thread n. At least one box needs to be assigned\\
        \inltt{RootOutputL2Norm}      & \xmark   & 0 &
        Root thread outputs the L2 norm of the physics values over the points if RootOutputL2Norm is 1.\\
        \inltt{FrameVelocity}      & \xmark   & 0 &
        The frame velocity which will be subtracted from the points' velocity.\\
        \inltt{IntOrder}      & \xmark   & 1 &
        Time integration order for points tracking. The points will be set as stationary if IntOrder is 0.\\
        \bottomrule
    \end{tabularx}
\end{center}

An example is given below:
\begin{lstlisting}[style=XMLStyle]
  <FILTERS>
    <FILTER TYPE="LagrangianPoints">
      <PARAM NAME="OutputFile">Points</PARAM>
      <PARAM NAME="OutputFrequency">10</PARAM>
      <PARAM NAME="Box_0">0, 1,32,0.3,0.6,0.0,0.49</PARAM>
      <PARAM NAME="Box_1">32, 1,32,0.3,0.6,0.51,1.0</PARAM>
      <PARAM NAME="RootOutputL2Norm">1</PARAM>
    </FILTER>
  </FILTERS>
\end{lstlisting}
